***No-Till Drill Information Sheet***

Drill Specifications: Truax FLXII-88 Warm Season Drill.

Drill is 8 feet wide (outside tires), has 8 planting rows, 8" spacing. Plants 5 .3' per pass with seeds planted 1/2" deep.

Mechanical Requirements: The drill has a tongue style hitch.

Minimum of a 35 horse power tractor with a hydraulic hook-up is required. The drill has standard Pioneer hydraulic couplers or John Deere hydraulic quick couplers.

Seedbed Preparations: The drill works best on dry, untilled soil. If the soil has been worked up, rolling the ground prior to planting with a culipacker or similar device is highly recommended. Use herbicide according to label directions for weed control.

Planting Ability: **(KEEP WILDFLOWER SEED, SEPARATE FROM GRASS SEED)**

Three seed boxes on the drill with independent rate adjustment for each box.

From front of the drill to the back: 1) Small seed box, 2)Warm season (fluff) seed box, 3) Cool season seed box.

Seed delivery is a straight line drop from seed boxes to the double disc openers. The rolling disc opener carries the seed into the ground for the best possible placement.

1. Small Seed, Seed Box: gravity flow seeds. Examples: Clover, Alfalfa,

Switchgrass ( only if pure switchgrass ), wildflowers.

1. Medium Seed (fluffy), Seed Box: Fluffy, bearded, awned seeds that will not gravity flow .. Primary Sideoats Grama, Wildflowers, and Native Prairie Seed Mix. Metal auger presses seed for accurate flow.
2. Large Seed, Seed Box: gravity flow seeds. Examples: Oats, Pasture grass seedings (grass/clover mixes), Food Plots, Nesting Cover Mixes. Metal agitators and metal fluted feed metering system.